| Opcode           | Instruction     | Op/En | 64-Bit Mode | Compat/Leg Mode | Description                      |
| ---------------- | --------------- | ----- | ----------- | --------------- | -------------------------------- |
| D0 /4            | SAL r/m8, 1     | M1    | Valid       | Valid           | Multiply r/m8 by 2, once.        |
| REX + D0 /4      | SAL r/m82, 1    | M1    | Valid       | N.E.            | Multiply r/m8 by 2, once.        |
| D2 /4            | SAL r/m8, CL    | MC    | Valid       | Valid           | Multiply r/m8 by 2, CL times.    |
| REX + D2 /4      | SAL r/m82, CL   | MC    | Valid       | N.E.            | Multiply r/m8 by 2, CL times.    |
| C0 /4 ib         | SAL r/m8, imm8  | MI    | Valid       | Valid           | Multiply r/m8 by 2, imm8 times.  |
| REX + C0 /4 ib   | SAL r/m82, imm8 | MI    | Valid       | N.E.            | Multiply r/m8 by 2, imm8 times.  |
| D1 /4            | SAL r/m16, 1    | M1    | Valid       | Valid           | Multiply r/m16 by 2, once.       |
| D3 /4            | SAL r/m16, CL   | MC    | Valid       | Valid           | Multiply r/m16 by 2, CL times.   |
| C1 /4 ib         | SAL r/m16, imm8 | MI    | Valid       | Valid           | Multiply r/m16 by 2, imm8 times. |
| D1 /4            | SAL r/m32, 1    | M1    | Valid       | Valid           | Multiply r/m32 by 2, once.       |
| REX.W + D1 /4    | SAL r/m64, 1    | M1    | Valid       | N.E.            | Multiply r/m64 by 2, once.       |
| D3 /4            | SAL r/m32, CL   | MC    | Valid       | Valid           | Multiply r/m32 by 2, CL times.   |
| REX.W + D3 /4    | SAL r/m64, CL   | MC    | Valid       | N.E.            | Multiply r/m64 by 2, CL times.   |
| C1 /4 ib         | SAL r/m32, imm8 | MI    | Valid       | Valid           | Multiply r/m32 by 2, imm8 times. |
| REX.W + C1 /4 ib | SAL r/m64, imm8 | MI    | Valid       | N.E.            | Multiply r/m64 by 2, imm8 times. |
